ESB32 Algorithm

1-open Arduino IDE .

2-Open File > Preferences.

3-click and "Manage the handling of additional plates" (https://dl.espressif.com/dl/package\_esp32\_index.json).

4-Open tools > "Arduino Uno" board >board manager.

5-Find ESP 32 and click it.

6-install the ESP32.

7- Connect the ESB32 to USB cable.

8-Open tools > "Arduino Uno" board > ESP32 Arduino > choose ESP32 type.

9- Change port to "COM3"

10- Program the code.

11-load the code by upload button.